; Unit conversion factors for use with Visio IntelliCAD
;
; ZwCAD.unt
; Release 1.0
;
; .............................................................................
;
; Copyright (c) 1998 by Visio Corporation.  All rights reserved.
;
; The Software is subject to the license agreement that accompanies
; or is included with the Software, which specifies the permitted
; and prohibited uses of the Software.  Any unauthorized duplication
; or use of Visio Corporation Software, in whole or in part, in print,
; or in any other storage and retrieval system is prohibited.
;
; To the maximum extent permitted by applicable law, Visio Corporation
; and its suppliers disclaim any and all warranties and conditions,
; either express or implied, including, without limitation, implied
; warranties of merchantability, fitness for a particular purpose,
; title, and non-infringement, and those arising out of usage of trade
; or course of dealing, concerning these materials.  These materials
; are provided "as is" without warranty of any kind.
;
; .............................................................................
;
; Sources:
;
;   "CRC Handbook of Chemistry and Physics, 52nd Edition 1971-1972",(c) 1971
;   "Physics, Parts I and II", by David Halliday and Robert Resnick (c) 1966
:   "The Astronomical Almanac, 1992", U.S. Government Printing Office (c) 1991
;
; .............................................................................
;
; Fundamental units are defined in terms of five fundamental physical
; constants, expressed in AI units.  From the CRC Handbook,
; pp. F189-F190:
;
;   c : The vacuum speed of light
;         2.9979250E+08 m/sec
;
;   e : Electron charge
;         1.6021917E-19 C (coulombs)
;
;   h : The Planck Constant
;         6.626196E-34  kg-m^2/sec
;
;   k : The Boltzmann Constant
;         1.380622E-23 kg-m^2/sec^2-K (K=degrees kelvin)
;
;   m : Electron rest mass (kg)
;         9.109558E-31 kg
;
; A line defining a unit in fundamental form has the form
;
;   x1,x2,x3,x4,x5,f,a
;
; The "x" terms are (integer) exponents of the five fundamental
; constants; "f" is a factor; "a" is an additive term (used only in
; temperature).  They define a value as follows (where ^ denotes
; exponentiation and * multiplication):  If we have U of the units
; being defined, the AI equivalent is
;
;   (c^x1 * e^x2 * h^x3 * k^x4 * m^x5) * (U*f + a)
;
; Notice that the factor composed of the fundamental constants defines
; a "fundamental unit" that is some multiple of the corresponding
; AI unit.  If we have U of the units we're defining, we therefore
; have U*f+a "fundamental units".  To convert this to some other unit,
; we seek U', where U'*f'+a' = U*f+a, or
;
;   U' = (U*f+a-a')/f'
;
; For all but temperature, a and a' are zero reducing this to
;
;   U' = U*f/f'
;
; Because of the way we're combining the fundamental constants to
; produce a specific type of unit via dimensional analysis (length,
; mass, speed, etc.), all fundamental definitions of the same type have
; the same set of exponents (x1-x5).  Here are the formats of some of
; the basic types (along with their "fundamental units" in AI units,
; using the CRC values):
;
;   Length:
;     -1, 0, 1, 0,-1,f,0 (2.426309557165E-12 m)
;   Mass:
;      0, 0, 0, 0, 1,f,0 (9.109558E-31 kg)
;   Time:
;     -2, 0, 1, 0,-1,f,0 (8.0932963872178E-21 sec)
;   Temperature:
;      2, 0, 0,-1, 1,f,a (5.9301276689232E+09 K)
;   Area:
;     -2, 0, 2, 0,-2,f,0 (5.8869780671902E-24 m^2)
;   Volume:
;     -3, 0, 3, 0,-3,f,0 (1.4283631147244E-35 m^3)
;   Speed:
;      1, 0, 0, 0, 0,f,0 (2.9979250E+08 m/sec)
;   Acceleration:
;      3, 0,-1, 0, 1,f,0 (3.7042076016576E+28 m/sec^2)
;   Force:
;      3, 0,-1, 0, 2,f,0 (3.374369399134E-02 kg-m/sec^2 (newton))
;   Pressure:
;      5, 0,-3, 0, 4,f,0 (5.7319211327461E+21 kg/sec^2-m (N/m^2))
;   Energy:
;      2, 0, 0, 0, 1,f,0 (8.1872647225241E-14 kg-m^2/sec^2 (joule))
;   Power:
;      4, 0,-1, 0, 2,f,0 (1.0116106380899E+07 kg-m2/sec^3 (watt))
;   Electric charge:
;      0, 1, 0, 0, 0,f,0 (1.6021917E-19 C (coulomb))
;   Electric current:
;      2, 1,-1, 0, 1,f,0 (1.9796528180167E+01 C/sec (amp))
;   Electromotive force:
;      2,-1, 0, 0, 1,f,0 (5.1100406540142E+05 kg-m^2/sec^2-C (volt))
;   Electric resistance:
;      0,-2, 1, 0, 0,f,0 (2.5812812264393E+04 kg-m^2/sec-C^2 (ohm))
;   Electric capacitance:
;     -2, 2, 0, 0,-1,f,0 (3.1353795566018E-25 sec^2-C^2/kg-m^2 (farad))
;   Electric inductance:
;     -2,-2, 2, 0,-1,f,0 (2.0891074024335E-16 kg-m^2/C^2 (henry))
;   Magnetic flux:
;      0,-1, 1, 0, 0,f,0 (4.1357073563669E-15 kg-m^2/sec-C (weber))
;   Magnetic induction:
;      2,-1,-1, 0, 2,f,0 (7.0251788084898E+8  kg/sec-C (tesla))
;   Dimensionless multiplier:
;      0, 0, 0, 0, 0,f,0 (No units)
;
; Excluding temperatures, we can combine these to produce composite
; units as follows:
;
;   To multiply any two of these, you add the exponents (x1-x5) and
;   multiply the f's.
;
;   To divide one by another, you subtract the second's exponents from
;   the first's and divide the first f by the second.
;
;   To raise one to a power, you multiply the exponents (x1-x5) by the
;   power and raise f to the power.
;
; In acad.unt, the "fundamental units" are those actually produced by
; combining the fundamental constants.  For example, the fundamental
; unit of length is h/(mc), which is 2.426309557165E-12 m, and we
; therefore need mc/h of these (4.1214856408036E+11) to make one meter.
; (This changes, of course, whenever one of the fundamental constant
; values is refined.  But, as long as we use the same values for
; source and destination units in the conversion, this doesn't matter.)
;
; Since we're only using these "fundamental units" as temporary
; intermediates for comparing different units of like type, why not
; use the SI units themselves as the "fundamental units"?  That's what
; icad.unt does in this file.  So, instead of
;
;   *meter(s),metre(s),m
;   -1,0,1,0,-1,4.1214856408036E+11,0
;
; we have
;
;   *meter(s),metre(s),m
;   -1,0,1,0,-1,1.0,0
;
; h/(mc) is indeed a length, but a very cumbersome one compared to
; a meter.
;
; The exponents remain the same, but their function is purely that
; of unit type-identifiers, making sure the dimensional analysis
; works out.  (Meters, Kilograms, Seconds, and Kelvins could be used
; in the same manner, but we keep the "c,e,h,k,m" system to maintain
; compatibility with ACAD.)
;
; .............................................................................
;
;     File format information:
;
; A semicolon begins a comment that continues through the end of the line.
;
; Blank lines are ignored.
;
; A unit definition has two lines:
;
;   The name(s) of the unit:
;
;     The line must begin with an asterisk.  Synonyms are separated by
;     commas.  Each synonym can have the form
;
;       prefix(singularsuffix.pluralsuffix)
;
;     The "singularsuffix." part can be omitted; so can the entire
;     parenthetical singular/plural item.
;
;   The definition:
;
;     One of the three following formats:
;
;       Fundamental format:
;
;         The "x1,x2,x3,x4,x5,f,a" format discussed earlier.
;
;       Derived format:
;
;         This type must begin with an equals sign (=), followed by
;         literal constants and the names of other defined units and
;         any of the math operators * (multiplication), / (division),
;         and ^ (exponentiation).  Multiplication is implied if no
;         operator is supplied between non-operator items.  Any
;         derived units used in the formula must of course be
;         resolvable to fundamental form using other definitions in
;         this file (in a non-recursive manner -- no infinite
;         definition loops!).
;
;         It seems ACAD only allows ONE division on a definition
;         line (or in a string passed to cvunit) -- probably because
;         that's how scientists generally write units: a bunch of units
;         over another bunch of units -- one division.  For example,
;         an acceleration in feet per second per minute must
;         be given as "ft / sec min", not "ft / sec / min".
;
;         The units are combined on each side of the slash,
;         and the division is performed last.
;
;         See acad.unt for examples of this format.  Icad.unt specifies
;         all of it's definitions in "fundamental" format.  This
;         allows cvunit to process this file faster, with fewer
;         calculations (and therefore smaller rounding errors).
;         Since icad.unt uses SI units as the fundamental units,
;         the file is fairly "human-readable": the "f" terms are
;         the SI equivalents -- not some collection of cumbersome
;         physical constants.
;
;       Exponent synonym definition format:
;
;         Of the form
;
;           *square,sq
;           ^2
;
;         Note there's no equals sign ("^2", not "=^2").
;
;         ACAD defines this one and "*cubic,cu", but doesn't use
;         them in acad.unt.  We follow suit.
;
;         If you DO use them, it seems they must appear BEFORE the
;         item to operate on, not after ("sq ft", not "ft sq").
;         However, if you use exponents directly, you must put them
;         AFTER the item ("ft^2").  Therefore, "sq" is not a direct
;         synonym for "^2".
;
;         We recommend using an exponent directly -- right up
;         against the item it follows (like "meter^3").
;
; .............................................................................


; Exponent definitions (See notes above.  They're NOT substitutions.)

*square,sq
^2

*cubic,cu
^3


; The primary SI units:

*meter(s),metre(s),m,centare(s)
-1, 0, 1, 0,-1,1.0,0.0

*kilogram(s),kg
 0, 0, 0, 0, 1,1.0,0.0

*second(s),sec
-2, 0, 1, 0,-1,1.0,0.0

*kelvin(s),k
 2, 0, 0,-1, 1,1.0,0.0

*ampere(s),amp(s)
 2, 1,-1, 0, 1,1.0,0.0

*candela,cd             ; Careful with this one.  This file (as shipped)
 4, 0,-1, 0, 2,1.0,0.0  ; does not specify any other luminous intensity
                        ; units.  If you add any, keep the exponents (x1-x5)
                        ; the same.  Enter the equivalent number of
                        ; candelas for f -- or replace the 1.0 in the
                        ; candela definition with the true MKS equivalent
                        ; and then enter others in terms of that MKS value.
                        ;
                        ; As it stands, THIS candela is equivalent to
                        ; a watt -- which I doubt is true.  (acad.unt
                        ; has the same problem.)

; Length:

*angstrom(s)
-1, 0, 1, 0,-1,1.0E-10,0.0

*astronomical_unit(s),au
-1, 0, 1, 0,-1,1.49597870E+11,0.0

*bolt(s)
-1, 0, 1, 0,-1,36.576,0.0

*cable(s)
-1, 0, 1, 0,-1,219.456,0.0

*centimeter(s),centimetre(s),cm
-1, 0, 1, 0,-1,0.01,0.0

*chain(s) ; Gunter's
-1, 0, 1, 0,-1,20.1168,0.0

*cubit(s)
-1, 0, 1, 0,-1,0.4572,0.0

*decimeter(s),decimetre(s),dm
-1, 0, 1, 0,-1,0.1,0.0

*dekameter(s),decameter(s),dekametre(s),decametre(s),dam
-1, 0, 1, 0,-1,10.0,0.0

*fathom(s),fath
-1, 0, 1, 0,-1,1.8288,0.0

*foot,feet,ft,'
-1, 0, 1, 0,-1,0.3048,0.0

*furlong(s),fur
-1, 0, 1, 0,-1,201.168,0.0

*gigameter(s),gigametre(s)
-1, 0, 1, 0,-1,1.0E+09,0.0

*hand(s)
-1, 0, 1, 0,-1,0.1016,0.0

*hectometer(s),hectometre(s),hm
-1, 0, 1, 0,-1,100.0,0.0

*inch(es),in(s),"
-1, 0, 1, 0,-1,0.0254,0.0

*kilometer(s),kilometre(s),km
-1, 0, 1, 0,-1,1000.0,0.0

*league_nautical  ;  International
-1, 0, 1, 0,-1,5556.0,0.0

*league_statute
-1, 0, 1, 0,-1,4828.032,0.0

*lightyear(s),ly  ;  Using a tropical year
-1, 0, 1, 0,-1,9.4605281774268E+15,0.0

*link(s)  ;  Gunter's
-1, 0, 1, 0,-1,0.201168,0.0

*micron(s)
-1, 0, 1, 0,-1,0.000001,0.0

*mil(s)
-1, 0, 1, 0,-1,0.0000254,0.0

*mile_nautical,inm  ;  International
-1, 0, 1, 0,-1,1852.0,0.0

*mile(s),mile_statute,mi
-1, 0, 1, 0,-1,1609.344,0.0

*millimeter(s),millimetre(s),mm
-1, 0, 1, 0,-1,0.001,0.0

*millimicro(s),nanometer(s),nanometre(s)
-1, 0, 1, 0,-1,1.0E-09,0.0

*pace(s)
-1, 0, 1, 0,-1,0.762,0.0

*palm(s)
-1, 0, 1, 0,-1,0.0762,0.0

*parsec(s),pc  ;  From definition and the value of the astronomical unit.
-1, 0, 1, 0,-1,3.0856775670468E+16,0.0

*pica(s)
-1, 0, 1, 0,-1,0.0042175176,0.0

*point(s)
-1, 0, 1, 0,-1,0.0003514598,0.0

*rod(s)
-1, 0, 1, 0,-1,5.0292,0.0

*rope(s)  ;  British
-1, 0, 1, 0,-1,6.096,0.0

*skein(s)
-1, 0, 1, 0,-1,109.728,0.0

*span(s)
-1, 0, 1, 0,-1,0.2286,0.0

*survey_foot,survey_feet  ;  Based on the old standard of exactly 39.37 in/m.
-1, 0, 1, 0,-1,0.30480060960122,0.0

*yard(s),yd
-1, 0, 1, 0,-1,0.9144,0.0


; Mass:

*cental(s)  ;  British
 0, 0, 0, 0, 1,45.359237,0.0

*dalton(s)  ;  Chemistry
 0, 0, 0, 0, 1,1.66024E-27,0.0

*grain(s)  ;  (1/480 ounce_troy)
 0, 0, 0, 0, 1,6.4798929166666666666E-05,0.0

*gram(s),gm,g
 0, 0, 0, 0, 1,0.001,0.0

*hundredweight(s)  ;  Short (100 lb avdp)
 0, 0, 0, 0, 1,45.359237,0.0

*long_ton(s)  ;  (2240 lb avdp)
 0, 0, 0, 0, 1,1016.0469088,0.0

*microgram(s)
 0, 0, 0, 0, 1,1.0E-09,0.0

*milligram(s),mg
 0, 0, 0, 0, 1,0.000001,0.0

*ounce_troy
 0, 0, 0, 0, 1,0.031103486,0.0

*ounce_weight,ounce(s),oz
 0, 0, 0, 0, 1,0.028349523125,0.0

*pennyweight(s),dwt,pwt  ;  (1/20 ounce_troy)
 0, 0, 0, 0, 1,0.0015551743,0.0

*pound(s),lb(s) ; avdp
 0, 0, 0, 0, 1,0.45359237,0.0

*poundal(s)
 0, 0, 0, 0, 1,0.01409808,0.0

*scruple(s)  ;  Apothecary (1/24 ounce_troy)
 0, 0, 0, 0, 1,0.0012959785833333333333,0.0

*slug(s)
 0, 0, 0, 0, 1,14.5939,0.0

*stone(s)  ;  British
 0, 0, 0, 0, 1,6.35029318,0.0

*ton_metric,tonne(s)
 0, 0, 0, 0, 1,1000.0,0.0

*ton_short,ton(s)
 0, 0, 0, 0, 1,907.18474,0.0


; Time:

*calendar_year(s),year(s),yr
-2, 0, 1, 0,-1,31536000.0,0.0  ; Calendar -- 365 days
                               ; One could argue whether "year" should be
                               ; the calendar one or the tropical.
                               ; We follow ACAD for compatibility.

*century,centuries
-2, 0, 1, 0,-1,3153600000.0,0.0  ; Calendar -- 36500 days

*day(s)
-2, 0, 1, 0,-1,86400.0,0.0

*decade(s)
-2, 0, 1, 0,-1,315360000.0,0.0  ; Calendar -- 3650 days

*fortnight(s)
-2, 0, 1, 0,-1,1209600.0,0.0

*hour(s),hr(s)
-2, 0, 1, 0,-1,3600.0,0.0

*microsecond(s)
-2, 0, 1, 0,-1,0.000001,0.0

*millennium,millennia,millenium,millenia
-2, 0, 1, 0,-1,31536000000.0,0.0  ; Calendar -- 365000 days

*millisecond(s),msec
-2, 0, 1, 0,-1,0.001,0.0

*minute(s),min(s)
-2, 0, 1, 0,-1,60.0,0.0

*nanosecond(s),nsec
-2, 0, 1, 0,-1,1.0E-09,0.0

*sidereal_year(s)
-2, 0, 1, 0,-1,31558149.504,0.0

*tropical_year(s)
-2, 0, 1, 0,-1,31556925.216,0.0

*week(s),wk
-2, 0, 1, 0,-1,604800.0,0.0


; Frequency

*hertz,hz
 2, 0,-1, 0, 1,1.0,0.0


; Area:

*acre(s)
-2, 0, 2, 0,-2,4046.8564,0.0

*are(s)
-2, 0, 2, 0,-2,100.0,0.0

*barn(s)
-2, 0, 2, 0,-2,1.0E-28,0.0

*hectare(s)
-2, 0, 2, 0,-2,10000.0,0.0

*rood(s)  ;  British
-2, 0, 2, 0,-2,1011.7141,0.0

*township(s)
-2, 0, 2, 0,-2,93239571.456,0.0


; Volume:
;
;   Note: The US fluid values quart, pint, cup, ounce, and dram
;   are based on integral subdivisions of the gallon.  (The CRC
;   reference has an internal inconsistency between pint and ounce.)
;
;   The dry equivalents are also based on the subdivided gallon.

*barrel(s)  ;  US petroleum
-3, 0, 3, 0,-3,0.1589872956,0.0

*board_foot,board_feet
-3, 0, 3, 0,-3,0.002359737216,0.0

*british_gallon(s)
-3, 0, 3, 0,-3,0.004546087,0.0

*bushel(s),bu  ;  US
-3, 0, 3, 0,-3,0.03523907,0.0

*butt(s)  ;  British
-3, 0, 3, 0,-3,0.4769618868,0.0

*cc
-3, 0, 3, 0,-3,0.000001,0.0

*centiliter(s),centilitre(s)
-3, 0, 3, 0,-3,0.00001000028,0.0

*cord(s)  ;  128 ft^3 (This CRC value looks like it's based on survey feet.)
-3, 0, 3, 0,-3,3.6245734,0.0

*decaliter(s),*dekaliter(s),*decalitre(s),*dekalitre(s)
-3, 0, 3, 0,-3,0.01000028,0.0

*decastere(s),dekastere(s)
-3, 0, 3, 0,-3,10.0,0.0

*decistere(s)
-3, 0, 3, 0,-3,0.1,0.0

*dry_gallon(s)  ;  US
-3, 0, 3, 0,-3,0.0044048828,0.0

*dry_pint(s)  ;  US
-3, 0, 3, 0,-3,0.00055061035,0.0

*dry_quart(s)  ;  US
-3, 0, 3, 0,-3,0.0011012207,0.0

*fluid_cup(s),cup(s)  ;  US
-3, 0, 3, 0,-3,0.0002365882375,0.0

*fluid_dram(s),dram(s),dr  ;  US
-3, 0, 3, 0,-3,3.6966912109375E-06,0.0

*fluid_gallon(s),gallon(s),gal  ;  US
-3, 0, 3, 0,-3,0.0037854118,0.0

*fluid_ounce(s)  ; US
-3, 0, 3, 0,-3,2.95735296875E-05,0.0

*fluid_pint(s),pint(s)  ; US
-3, 0, 3, 0,-3,0.000473176475,0.0

*fluid_quart(s),quart(s),qt  ;  US
-3, 0, 3, 0,-3,0.00094635295,0.0

*firkin(s)  ;  US  (9 US fluid gallons)
-3, 0, 3, 0,-3,0.0340687062,0.0

*gill(s)  ;  US  (1/32 US fluid gallons)
-3, 0, 3, 0,-3,0.00011829411875,0.0

*hectoliter(s),hectolitre(s)
-3, 0, 3, 0,-3,0.1000028,0.0

*hogshead(s)  ;  (63 US fluid gallons)
-3, 0, 3, 0,-3,0.2384809434,0.0

*kilderkin(s)  ;  British
-3, 0, 3, 0,-3,0.08182957,0.0

*kiloliter(s),kilolitre(s)
-3, 0, 3, 0,-3,1.000028,0.0

*liter(s),litre(s)
-3, 0, 3, 0,-3,0.001000028,0.0

*milliliter(s),millilitre(s),ml
-3, 0, 3, 0,-3,0.000001000028,0.0

*minim(s)  ;  US  (1/60 US fluid dram (1/61440 US fluid gallon))
-3, 0, 3, 0,-3,6.1611520182292E-08,0.0

*peck(s)  ;  US  (2 US dry gallons)
-3, 0, 3, 0,-3,0.0088097656,0.0

*pottle(s)  ;  (0.5 British gallons)
-3, 0, 3, 0,-3,0.0022730435,0.0

*puncheon(s)
-3, 0, 3, 0,-3,0.31797510,0.0  ;  British

*register_ton(s)  ;  (100 ft^3)
-3, 0, 3, 0,-3,2.8316846592,0.0

*seam(s)  ;  (64 British gallons)
-3, 0, 3, 0,-3,0.290949568,0.0

*stere(s)
-3, 0, 3, 0,-3,1.0,0.0

*tun(s)  ;  (252 US fluid gallons (4 hogsheads))
-3, 0, 3, 0,-3,0.9539237736,0.0


; Speed:

*light_speed   ;  The new, exact, value (not the CRC one).
 1, 0, 0, 0, 0,299792458.0,0.0

*knot(s)  ;  Nautical miles / hr
 1, 0, 0, 0, 0,0.51444444444444444444,0.0


; Acceleration:

*g_acceleration
 3, 0,-1, 0, 1,9.80665,0.0


; Force:

*dyne(s)
 3, 0,-1, 0, 2,0.00001,0.0

*force_pound(s)
 3, 0,-1, 0, 2,4.4482216765935,0.0

*newton(s)
 3, 0,-1, 0, 2,1.0,0.0


; Pressure:

*atmosphere(s),atm
 5, 0,-3, 0, 4,101325.0,0.0

*bar(s)
 5, 0,-3, 0, 4,100000.0,0.0

*barye(s)
 5, 0,-3, 0, 4,0.1,0.0

*pascal
 5, 0,-3, 0, 4,1.0,0.0

*torr(s),mm_of_hg
 5, 0,-3, 0, 4,133.32236842105,0.0


; Energy:

*british_thermal_unit(s),btu(s)
 2, 0, 0, 0, 1,1054.35,0.0

*calorie(s),cal  ;  Gram-calorie
 2, 0, 0, 0, 1,4.184,0.0

*joule(s)  ;  Absolute (kg-m^2/sec^2)
 2, 0, 0, 0, 1,1.0,0.0

*kilocalorie(s),kcal  ;  Kilogram-calorie (the nutritional calorie)
 2, 0, 0, 0, 1,4184.0,0.0

*electron_volt(s),ev
 2, 0, 0, 0, 1,1.60209E-19,0.0

*erg(s)
 2, 0, 0, 0, 1,1.0E-07,0.0


; Power

*horsepower,hp
 4, 0,-1, 0, 2,745.700,0.0

*kilowatt(s),kw
 4, 0,-1, 0, 2,1000.0,0.0

*watt(s),w
 4, 0,-1, 0, 2,1.0,0.0


; Electric charge:

*coulomb(s)
 0, 1, 0, 0, 0,1.0,0.0

*electron_charge(s)
 0, 1, 0, 0, 0,1.60209E-19,0.0


; Electric current:

*microampere(s),microamp(s)
 2, 1,-1, 0, 1,0.000001,0.0

*milliampere(s),milliamp(s),ma
 2, 1,-1, 0, 1,0.001,0.0


; Electromotive force:

*volt(s),v
 2,-1, 0, 0, 1,1.0,0.0

*millivolt(s),mv
 2,-1, 0, 0, 1,0.001,0.0

*microvolt(s)
 2,-1, 0, 0, 1,0.000001,0.0


; Electric resistance:

*ohm(s)
 0,-2, 1, 0, 0,1.0,0.0


; Electric capacitance:

*farad(s)
-2, 2, 0, 0,-1,1.0,0.0


; Electric inductance:

*henry,henries
-2,-2, 2, 0,-1,1.0,0.0


; Magnetic flux:

*maxwell(s)
 0,-1, 1, 0, 0,1.0E-08,0.0

*weber(s)
 0,-1, 1, 0, 0,1.0,0.0


; Magnetic induction:

*gauss(es)
 2,-1,-1, 0, 2,0.0001,0.0

*tesla(s)
 2,-1,-1, 0, 2,1.0,0.0


; Angle

*arc_minute(s)
 0, 0, 0, 0, 0,60.0,0.0

*arc_second(s)  ;  Used as the fundamental angular unit.
 0, 0, 0, 0, 0,1.0,0.0

*circle(s)
 0, 0, 0, 0, 0,1296000.0,0.0

*degree(s),deg
 0, 0, 0, 0, 0,3600.0,0.0

*grad(s)
 0, 0, 0, 0, 0,3240.0,0.0

*quadrant(s)
 0, 0, 0, 0, 0,324000.0,0.0

*radian(s)
 0, 0, 0, 0, 0,206264.80624709636,0.0


; Solid angle

*hemisphere(s)
 0, 0, 0, 0, 0,6.28318530717958647692,0.0

*sphere(s)
 0, 0, 0, 0, 0,12.56637061435917295384,0.0

*steradian(s)
 0, 0, 0, 0, 0,1.0,0.0


; Dimensionless multiples and submultiples:

*atto
 0, 0, 0, 0, 0,1.0E-18,0.0

*centi
 0, 0, 0, 0, 0,0.01,0.0

*deca,deka
 0, 0, 0, 0, 0,10.0,0.0

*deci
 0, 0, 0, 0, 0,0.1,0.0

*exa
 0, 0, 0, 0, 0,1.0E+18,0.0

*femto
 0, 0, 0, 0, 0,1.0E-15,0.0

*giga
 0, 0, 0, 0, 0,1.0E+09,0.0

*hecto
 0, 0, 0, 0, 0,100.0,0.0

*kilo
 0, 0, 0, 0, 0,1000.0,0.0

*mega
 0, 0, 0, 0, 0,1.0E+06,0.0

*micro
 0, 0, 0, 0, 0,1.0E-06,0.0

*milli
 0, 0, 0, 0, 0,0.001,0.0

*nano
 0, 0, 0, 0, 0,1.0E-09,0.0

*peta
 0, 0, 0, 0, 0,1.0E+15,0.0

*pico
 0, 0, 0, 0, 0,1.0E-12,0.0

*tera
 0, 0, 0, 0, 0,1.0E+12,0.0
